MTMS Alarm Check
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To check MTMS alarms, select Failures Insert from Custom Usual Options or from the Maintenance menu.
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Stat the number using the FNN (without the leading zero) and then press Enter or the OK button.


If the tech only has the CAB ID, translate this number to the FNN using Plant Maintenance or AXIS. (or, if desperate, the cab ID can be put into the Maintenance / Reports section, but the above method is the preferred option).

Alarms are displayed showing alarm numbers,  descriptions 


and date & time of alarm generated. 





The upper part of the panel displays the coin tin status. 





The UI Blocking & Upper Door Open fields can be ignored.








