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Details:
· A procedure has been developed which will enable a plastic case Bluephone Network Board (Material No. 035061302, figure 3.), to be fitted into a Metal Case or Diamond Bluephone. 

· If converting a plastic case Bluephone Network Board for use in Metal case or Diamond Bluephones, follow the conversion procedure below.

· When  ordering a Bluephone Network Board from the store, material number 035061401 is to be quoted.

Field Procedure to be Adopted:

Procedure for mounting 03561302 into Plastic Bluephone:

1. If necessary, change the top screw from metal-thread (fine) to plastic-thread (coarse). See figure 2.

2. Sit the bottom edge of the board behind the lip in the case.

3. Use the coarse threaded screw to secure the top of the board to the case.

Procedure for mounting 03561302 into Metal case Bluephone (CT6+):

1. If necessary, change the top screw from plastic-thread (coarse) to metal-thread (fine).

2. Screw the enclosed threaded white plastic pillar (figure 2) tightly into the case at the top mounting point.

3. Sit the bottom edge of the board behind the lip in the case.

4. Loosely screw the top screw into the pillar.

5. Fit the bottom two M3 screws to hold the board in place without bending it.

6. Tighten the top screw to remove slack without damaging the thread in the pillar or bending the board.

Observe any special work instructions concerning the use of this board in the CT6+ case.

The Metal case Bluephone may have a black plastic insulating membrane fitted between the Network Board and the case (figure 1) of the phone. This membrane must be left in place when fitting a new Network Board. If no membrane is found in the phone, it will be necessary to install one.

Procedure for mounting 03561302 into Diamond case Bluephone (CT6D):

1. If necessary, change the top screw from metal-thread (fine) to plastic-thread (coarse).

2. Sit the bottom edge of the board behind the lip in the insulating tray.
3. Use the coarse threaded screw to secure the top of the board to the tray. 

The Diamond case Bluephone may have a black plastic insulating membrane fitted between the Network Board and the case of the phone. This membrane must be left in place when fitting a new Network Board. If no membrane is found in the phone, it will be necessary to install one.
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Figure 4

Network Board sitting in Metal case Bluephone
Insulating Membrane





Metal and Diamond case Network Board.
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(Viewed from rear)
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Figure 3


Plastic case Bluephone Network Board
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Plastic thread screw
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Figure 1


Metal and Diamond Case Network Board


035061401 (Viewed from rear)
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Figure 2
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