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This Information Brief contains important information that affects the processes our people use.

Modified Longitudinal Surge Protection Units

Purpose
Inform staff of the changes made to the Longitudinal Surge Protection Unit 035/01299.

Background
Because of its firing voltage tolerance, the 90V Gas Arrestor used in the first release of the Longitudinal Surge Protection Unit conducts when the Payphone receives a 50Hz meter pulse or an incoming ring. 

There is no problem with Payphones connected to 12kHz metering lines where no incoming calls are allowed and does not effect the polling functionality due to be released in the near future.



Current Revision
To rectify this problem all the stock in stores and future stock will now have a 230V Gas Tube Arrestor fitted in place of the 90V Gas Tube Arrestor.

The Longitudinal Surge Protection Unit (Revision 1) is now fitted with 1 x 230V Gas  Tube  Arrestor, 2 x 4 ampere (M205) Slow Blow Anti Surge Fuse and a 2.5mm Green/Yellow earth cable

How to Order
Material Number
Description
Quantity Per Order


035/01299
Surge Protection, Longitudinal
1


035/01056
Fuse, 4 ampere slow blow
10

Impact on Field Operations
Action is only required from Field Staff if an older version arrestor (90V) is found installed at a 50Hz metering site or at a site where Incoming Calls are Allowed.  In this case the assembly should be changed to the 230V type.  If the fuses have blown they should be replaced with 4Ampere M205 Slow Blow Anti Surge Fuses.

Contact for further information
Tony Goldrick

Technical Product Manager

02 9329 0652
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