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This Information Brief contains important information that affects the processes our people use.

CT3H Display Protector

Purpose
To inform relevant staff that the Display Protector for the 200 prototype CT3H Payphones with the recessed display are available through the stores system.

Background
200 prototype CT3H Payphones were trialed in NSW and Victoria.  After the trial period, the Payphones were removed and placed in a refurbishment program.  The production models were built with the display flush with the facia, however, to save on costs the LCD mounting of the trial units was left in its recessed position. 

The prototype CT3H Payphones used the old CT3C/CP9 Payphone display protectors that are available under the original description and material number.

The 2,500 production CT3H Payphones differ, having a flush mounted display on a revised stainless steel facia for improved viewing.  The production CT3H Payphones use the standard Tsp/CT3H display protector 035/01152 (lexan) or 035/01641 (glass).

Changes made
The Description of the Material Number 035/02005 has recently been updated to reflect the current use of the material 

From:

035/02005 - WINDOW DISPLAY UNIT CP9

To:

035/02005 – WINDOW DISPLAY UNIT CT3H VERSION 1 (for recessed displays only)

This change will be updated on director in the next download.

How to Order
The Display Protector can be ordered from the stores system by quoting the material number for the part required


Material Number
Description
Quantity Per Order


035/02005
WINDOW DISPLAY UNIT CT3H VERSION 1
1

Contact for further information
Tony Goldrick

Technical Product Manager

02 9329 0652
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