PAYPHONES TESTS FROM SULTAN





Listed are TYPICAL responses that can be expected from SULTAN when testing the following payphones.





�
TSP�
CT3E


Coin only�
CT3C


Coin/card�
CP9


Card only�
CP8


credit�
BLUE		�
GOLD�
RED�
DTOP�
DORO�
�
A wire f batt�
0 volts�
0 volts�
0 volts�
0 volts�
0 volts�
0 volts�
0 volts�
0 volts�
0 volts�
0 volts�
�
B wire f batt�
0 volts�
0 volts�
0 volts�
0 volts�
0 volts�
0 volts�
0 volts�
0 volts�
0 volts�
0 volts�
�
A wire IR to eth�
>100M(�
>25M(�
>25M(�
16 M(�
>25M(�
>25M(�
>25 M(�
>25 M(�
>1.3 M(�
>25M(�
�
B wire IR to eth�
>100M(�
>25M(�
12M(�
8 M(�
>25M(�
>25M(�
>25M(�
>25M(�
>1.3 M(�
>25M(�
�
A to B wire IR�
>5M(�
1.3M(�
60 K(�
2.3 M(�
143M(�
50 K(�
47 K(�
2.3 M(�
>500 K(�
>5M(�
�
B to A wire IR�
>5M(�
1.3M(�
60 k(�
2.3 M(�
143M(�
50 K(�
47 K(�
2.3 M(�
>500 K(�
>5M(�
�
A wire cap.�
1.5 uf�
1.7 uf�
1.7 uf�
1.2 uf�
1.4 uf�
1.9 uf�
1.7 uf�
1.3 uf�
1.5 uf�
1.21 uf�
�
B wire cap.�
1.5 uf�
1.7 uf�
2.6 uf�
1.2 uf�
1.4 uf�
1.6 uf�
1.7 uf�
1.3 uf


�
1.5 uf�
1.21 uf�
�
INDIVIDUAL TEST MENU


This is available to testers after SULTAN has completed its initial line tests,


To access  -  dial 2 after hearing results of DC tests.





		     CODE	                    	        SULTAN TEST


Foreign Battery


Resistance / Capacitance test


Insulation resistance to Earth


Insulation resistance (A to B)


Open Circuit / Distance test


TSP, CT3E & CT3C = X1 & 2 - Z1 & 2.  BLUE = L3, 4, 5 & 6. GOLD = C3 & 4. DTOP = F1 & 2.








