Testing Of Lines Showing As “Special Number”

[image: image1.png]jnumber to be tested ? 0740519091

JACCESSING CRSE AXE NODE - PLEASE WAIT ...

[EXCHANGE SWITCHING STAGE — CRSXH

IDEVICE STATE DETAILS
STATE BLS FTYPE ADM ABS  SNB SNBST  LIST
BUSY H'@ 0740519091 BUSY

JAXE POTS SERVICE

INO REVERTIVE CALL TO THIS TEST POSITION

[ACCESSING MRT 27777, MTU 27011, PLEASE WAIT ...

[NOTE THAT AXE-MTU MAY NOT PERFORM ALL MEASUREMENTS IF IT HAS FOUND A PREVIOUS
VALUE OUT OF RANGE. SUCH MEASUREMENTS DISPLAY ‘NO RESULT

Inurber to be tested ? ||

NUM



[image: image2.png]5 4: CAM AXE ITI

Setting up the site log file.

ITI: call successful

CRSELODiK-——E 020515  AT-10 TIME 020516 1842 PAGE

35C0-F14, 1P=141.168.15.167;
USERID-C737744,HOME_SERUER-U3bCO-Fid, IP-14].168.18'.167

<

JSUSCC: SNB=0740519091 , SCL=LIE-0;
{oI e T'R 9600 Baudls 10G11 B Full dpx § Block ENZZIISTY INSERT B UTZ0Y




When unable to test a payphone line due to it being a “Special Number”, under certain conditions a test can be performed.
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This can be achieved in CAM AXE by removing the LTE-1 category, performing the test and replacing the LTE-1 category, as described below.


In CAM terminal mode, use the command line format SUSCC:SNB=nnnnnnnnnn,SCL=LTE-0;.

The line can now be tested.

After testing, replace the LTE-1 category in CAM terminal mode, using the command line format SUSCC:SNB=nnnnnnnnnn,SCL=LTE-1;.


