Allocation Of  SEPRM’s

This falls into the “sometimes works” category!!

From Sultan, determine the Node and Exchange Switching Stage.
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Network Operations - GOC

TMGHELP Test Site "Under Development"

For more information Contact : Dasren Cook

@ Edison (QLD) AXE TMG Details
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Upgrade Pending July 2001
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Use the link http://praise.pno.telecom.com.au/~emgsurvey/index.htm to go to the TMGHELP screen to display the desired SEPRM range.
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Select the appropriate State.

Choose the required node. (eg FRTB)
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Select the desired Switching Stage


LI3 ranges are displayed.


SEPRM ranges are displayed for SEPRM2 & SEPRM1.

Select desired SEPRM range (eg 128&&191).

Using CAM terminal mode, display the SEPRM range to determine which are in use (idle) and which are available (MBL).



Choose one of the SEPRMs in MBL state to be used to connect to the LI3. Check and program accordingly.

