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This is want the categories for TRITEL Payphones should be in CAM.

As follows:
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Line Type:
ELR – Wholesale Payphone

Access: 

NA6


Carrier:
 
NAAAP


TCL VALAUES:



TCL – 12



TLI – 4

When a fault presents itself, all test results and category changes must be recorded in the Splus scratch pad.

