<Ripped by Subby>

"REMOTE EXCHANGE TESTER"

OPERATOR GUIDE

1.    Dial Access number.

2.    Listen for "Remote Exchange Tester, ABC..." where ABC... Is the LRD Code.

3.    Listen for "Please enter PIN".


Enter the four digit PIN. If the PIN is invalid, the R.E.T. responds 
"Error, invalid PIN, please re-enter PIN". A maximum of three attempts is 
allowed.

4.    Listen for "Enter test line number".


Enter the number of the R.E.T. Test line (01-10)to be tested.

5.    If the Test line is not physically connected, the R.E.T. responds "Error, 
no line connected". If the Test line is connected, listen for "Line nn 
accessed".

6.    You are now able to perform any of the following tests (see 'Test 
Procedures and Commands', next page):

- Make an outgoing call and follow-on calls.

- Camp on the Test line and answer an incoming call.

- Answer an incoming call to the Test tine.

- Activate or de-activate "EASYCALL" or "CENTEL" facilities.

- Hang up the Test line and re-loop the same line or select another Test line.

- Perform a Hook Flash during an established call.

- Set the unit to Decadic mode

7.    Press # * # to end the test session. Listen for "Thank you".

8.    Hang up telephone.

Note: Difficulty in entering DTMF commands may be encountered after a connection has been made to a "TCARS". The 820 Hz test tone from the 'TCARS' tends to mask the DTMF to the R.E.T. The # * command should be entered during the silence period to ensure reliable detection.

TEST PROCEDURES AND COMMANDS

Outgoing calls

When the Test line dial tone is heard, simply dial the required number. 'Follow-on' calls can be made using the 'Line Re-loop' facility,

Command: nn nnnn nnnn...

Incoming Call Answer

Dial the actual telephone number of a Test Line and listen for ring tone. From another telephone, Log on to the R.E.T. and select the R.E.T. Test line number that is ringing. The two calls should be connected together.

Command: 
nn nnnn nnnn... (Test line number)



nn nnnn nnnn,.. (Access line)



pppp (PIN)



nn (R.E.T. Test line number)



Verify connection,

Camp on/Answer

To camp a call on to a Test line, select a Test line and press # * 22. Listen for "Camped on line nn". The R.E.T. is then ready to answer and connect an incoming call to the Test line.

Command: # * 22

Line Re-loop and Test Line Select

Pressing # *nn, where nn is the Test line number (01-10), will re-loop the line or loop the Test line selected. The R.E.T responds "Line nn accessed" for confirmation before dial tone is heard.

Command: # * nn, where nn = 01 -10

"EASYCALL" and "CENTEL"

Simply enter the appropriate command to program, activate or de-activate a special calling facility,

Command: * 21 03 9758 5933 #, listen for facility tone. (Example to activate Call Diversion)

Hook Flash

Pressing 0 * during an established call, will cause the R.E.T. to perform a 'timed loop break' or 'Hook Flash' preset to 90 ms, on the Test line. The Hook Flash can be used to set up a Malicious Call Trace. Another example to verify correct operation may be to set up a Test line for the 'Call waiting' facility, to access that Test line and place another call to that line. When the call waiting tone is heard on the Access line press 0 * to perform a hook flash, then press 2 (as per "EASYCALL" instructions) to take the call waiting.

Command: Establish call, press 0 *.

DTMF to Decadic Conversion

To test the Decadic function of the telephone exchange, select a Test line and enter # * 62. Listen for "Decadic mode, line nn, enter number followed by hash". When the number is received and the closing # is entered, the R.E.T. re-loops the Test line and dials the number in decadic. If no hash is entered, after 20 seconds, the R.E.T. dials the number entered.

Command: 
# * 62

nn nnnn nnnn... #.

Forced Disconnect

To end the test session, you may press # * # which commands the R.E.T. to hang up the Access line and Test line. The RET will also timeout automatically if no DTMF is detected within a 90 second period.
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