How to set up a test position

Example: to connect SAI-25 to monitor line no 02 93959480

1.  EXTPP:SURVEY;     Examine the print to find the next spare AT device, eg AT-120

2.  IOIOI:IO=AT-120; or whatever you next spare is.

3.  IOBLE:IO=AT-120;

4.  EXDRP:DEV=SAI-25; Check that the route name is something like S+PYNJA where PYNJA is the RSS name.

5.  EXROP:R=T+emg;   check to see the test route exists. If it doesn't then 

    EXROI:R=T+emg,DETY=TCALT,FNC=3; where emg is the EMG name.

6.  Make a note of the ATdevice that you are connected to. If in doubt, send Cntl+D to log off, and 

    press ENTER to log on. The AT number is in the header. Eg AT-7

7.  IMLCT:SPG=0;

8.  MCDVP:IO=AT-7;   or whatever your AT is.  Make a note of the NTN value in the printout.

9.  MCDVR:IO=AT-7;

10. MCDVI:IO=AT-120,NTN=ntn;  NTN is the number you made a note of at step 8.

11. END;

12. send Cntrl+d, press enter. You will now be logged on as AT-120.

13. EXTPI:BNB=0293959480,R=T+PYNJA;  or whatever your route name is.

14. EXATI;

You connection is now made. You should now restore the AT to how you found it.

15. IMLCT:SPG=0;

16. MCDVR:IO=AT-120;    or whatever your AT is.

17. MCDVI:IO=AT-7,NTN=ntn;   ntn is the number you made a note of at step 8.  This restores your 

    AT to original.

18. END;

19. Cntrl+D, ENTER. You will now be logged on as your original AT found in step 6.

20. IOBLI:IO=AT-120;   your new AT selected at step 1

21. IOIOR:IO=AT-120;  remove your AT selected at step 1.

