MTMS Specifics Change

This screen provides access to perform changes to parameters to allow incoming calls, make the payphone card only, etc for individual payphones.
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Access is from the Plant Maintenance screen.
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Select/De-select Coin usage




Permit/Bar Incoming Calls

The HPPC/Chipper should be de-selected at installation.

If access to the Parameter and Statistics menus is required to be restricted, the 4 digit password can be changed in this screen.
