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NEC DSLAM AM3x Platform Information

We have two types of DSLAM installed

AM31 DSLAM. 

These are rack mounted and installed in large exchange installations with a maximum of 2304 customers per DSLAM. 
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AM31's are installed as Access Hubs, ie with directly connected customers, or as Dedicated Hubs,  ie only has subtended AM31/AM35 DSLAMs., or as a subtended DSLAM off a AM31 dedicated hub

AM35 DSLAM. 

These self contained units and are installed in small exchanges with a maximum of 160 customers and RIM housings with a maximum of 96 customers.
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AM35's are always installed as subtended units off a AM31 dedicated hub.

AM31 Access Hub

Exchange rack mounted. Always connected via 155 Meg Optical

Four card types are installed, 

Controller card, IGUx. Integrated Gateway Unit optical controller card

Line Termination card LTUx. These are 48 port ADSL line termination cards.

Bus Extension card. BEU. This extends controller bus into electrically expanded subracks

ADSL Filter Card . This is the ADSL/PSTN filter card.

Controller card

Hardware types
Firmware Version (SR28)
NEC Part Number

IGU-A155-SH5
V2_17_14
E5853A

IGU-A155-LH5
V2_17_14
E5853B

IGU-A155-5
V2_17_14
E5853D

IGU-2A155
V2_17_14
E4014E

LTU card

Hardware types
Firmware Version (SR28)
NEC Part Number

LTU-48ADSL
V1_24_00 
E5881A

LTU-48ADSL-2

V1_40_00
E5881B

Bus Extension card

Hardware types
Firmware Version (SR28)
NEC Part Number

BEU-3
V3_17_06
R5737A

Filter card

Hardware types
Firmware Version (SR28)
NEC Part Number

FTU
N/A
R5886A

AM31 Dedicated Hub

Exchange rack mounted. Always connected via 155 Meg Optical

Four card types are installed, 

Controller card, IGUx. Optical controller card. Same as AM31 Access hub

Line Termination card LTUx. These are Subtending termination cards, IMA and Optical subtending cards.

Bus Extension card. BEU. Same card types as AM31 Access hub

ADSL Filter Card . This is the ADSL/PSTN filter card. Same as AM31 Access hub.

LTU card

Hardware types
Firmware Version (SR28)
NEC Part Number

LTU-8E1-IMA
V1_15_00
R5845A

LTU-4A155
V1_02_04
E5758B

AM31 Subtended

Exchange rack mounted. Connected by up to 8 x E1 IMA links

Four card types are installed, 

Controller card, IGUx. IMA connected controller card. 

Line Termination card LTUx. These are 48 port ADSL line cards. Same as AM31 Access hub

Bus Extension card. BEU. Same card types as AM31 Access hub

ADSL Filter Card . This is the ADSL/PSTN filter card. Same as AM31 Access hub.

Controller card

Hardware types
Firmware Version (SR28)
NEC Part Number

IGU-8E1-IMA-2
V2_17_11
E5959A

IGU-8E1-IMA-3
V2_17_28
E4015B

AM35 Subtended

Installed in Small exchanges and RIM housings

Three unit types are installed.

Base Unit. This unit contains an IGU controller card and one 32 port ADSL LTU card. Base Units are connected via 155Meg Optical or up to 8 x E1 IMA links

Expansion unit. This contains one 32 port ADSL LTU card. 

Filter unit. . This is the ADSL/PSTN filter card

Base Unit

Hardware types
Firmware Version (SR28)
NEC Part Number

AM35-I8E1-IMA
V2_17_11
E5914A

AM35-I8E1-IMA-2
V2_17_11
E5914C

AM35-I8E1-IMA-3
V2_17_14
E5914D

AM35-I155
V2_17_06
E5915C

AM35-I2A155
V2_17_14
E5915D

Expansion Unit

Hardware types
Firmware Version (SR28)
NEC Part Number

LTU-32ADSL-3
V1_38_01
E5922A

LTU-32ADSL-4
V1_50_00
E5922B

Filter Unit

Hardware types
Firmware Version (SR28)
NEC Part Number

FTU
N/A
E5923A

