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	AUDIENCE
	· Payphone Field Work Force Officers

· Team Leaders




This Information Brief contains important information that affects the processes our people use.

Water repel lube (CRC 5.56) use in Payphones
	Purpose
	To inform staff of the application of the lubricant CRC 5.56 in the Tsp & CT3H payphones.

	Background
	The chemical CRC 5.56 is already available for field staff to use.

It comes in a non-aerosol pump pack in two sizes.

This information brief will explain where it can be used in the payphones.

	Where CRC 5.56 can be used
	CRC 5.56 can be used to lubricate, inhibit corrosion and ease movement of all the metal pivot points (moving parts). Lock mechanisms, hinges, nuts and bolts are some examples where it can be used.

Do not under any circumstances use CRC 5.56 on any of the printed circuit boards or components (eg: validator, escrow) of the Tsp or the CT3H. Do not spray CRC into the lock barrel.

	How to Order
	The items can be ordered via the stores system by quoting the Material Number for the item required

	
	Material Number
	Description
	Quantity Per Order

	
	050/00040
	Water repel lube, penetrant pump type 1 litre


	1

	
	050/00041
	Water repel lube, penetrant pump type 0.5 litre


	1

	Impact on HS&E requirements
	Refer to Telesafe ID 4711 for further information and MSDS.

Although the product is a potentially a high-risk chemical, it is suitable for use, provided the user:

· reads the safety data sheet and if appropriate the label, 

· assesses the risks involved in using the product (unless already done so) 

· obtains adequate instruction in the use of the product, and follows the recommendations for safe use for this product.

	Contact for further information
	Perry Herbert

Telstra Payphones 

Technical support 

1800 815 804
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