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AUDIENCE
· Field Work Force

· Technical Specialist


This Information Brief contains important information that affects the processes our people use.

CT3H - PLATE, MOUNTING PBA  E-SHUTTER CONTRL CBLE
Purpose
A new material number has been created for mounting the PBA E Shutter Control Cable Plate

Background
The mounting plate is included with the CT3H E Shutter Housing (035/01595) (except for the first several hundred) when ordered for installation, but a separate material number is required for Service Assurance purposes.

The plate is used to mount the interconnection board, which is a component of the CT3H E‑SHUTTER EXTENSION CABLE (035/01596),.  This places the connectors on the interconnection board in a clear area to avoid possible damage that may be caused when lifting the Escrow/Validator Mounting Frame.

Installation Procedure
Refer to Work Instruction TPS1012-WS01 CT3H E Shutter Installation

How to Order
The Mounting Plate can be ordered by quoting the Material Number in the Table below


Material Number
Description
Quantity per Order


035/01654
PLATE, MOUNTING PBA E-SHUTTER CONTRL CBLE
1

Contact for further information
Tony Goldrick

Technical Product Manager

02 9329 0652
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