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AUDIENCE
· Field Work Force

· Technical Specialist


This Information Brief contains important information that affects the processes our people use.

Cables for Data Communications on Arunta Controlled Telephone Systems (ACTS)

Purpose
To inform IS staff on new cable options which are available for Data Communications on the ARUNTA Controlled Telephone system .

Background
The original data cabling used on installation activities for the RS 485 data network communication is becoming difficult to obtain. Therefore it has been decided to source a more modern and easily available cable.

Current Situation
Existing Cable- (2 types)

· Indoor Type

 The original standard sheath (non waterproof) cable  (Serial / Item 35/1058) is  no   longer available.                                                        

· Outdoor Type

          Waterproof polyethylene sheath cable (Serial / Item 35/1553) is no longer available. 

Replacement Cable

· Indoor Type

1. Service Operations staff and their contractors should use ISDN Cable: Digital Multi-Pair Balanced Screened Station Cable available through Telstra stores on (Serial/Item 353/750) under Contract 800030  Item number 90. This will replace (Serial /Item 35/1058).

2. An option is to use Cat5E STP (Shielded Twisted Pair). This cable is also a good match for the ACTS RS 485 network but is not a current serial and item through Telstra. Please obtain direct from Pirelli cables and quote part number L4P5ECS.

· Outdoor Type

Service Operations staff and their contractors should use Cat5E STP with waterproof polyethylene sheath and EMI  barrier as aluminium screen. The cable is also a good match for the ACTS RS 485 network but is not a current serial and item through Telstra. When sourcing the cable, allow the delivery time up to 12 weeks.

Installation Practice
There are no changes to any procedures in relation to installation techniques. All current cabling identification and labelling practices should be adhered to including the correct use of the appropriate colour heat shrink.

Contact for further information
Henry Tran

Telstra Payphone Services

Technical Support

02 9329 0634


Page 1 of 1

