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This Information Brief contains important information that affects the processes our people use.

Tsp1/CT3H Surge Protection Unit Replacement Fuse

Summary
A higher rated replacement fuse is to be used in the surge protection unit (material number 03501299) installed in Tsp1 and CT3H payphones.

Why?
The initial supply of Tsp1/CT3H Surge Protection Units material number 03501299 were fitted with 2 Amp Slow Blow Fuses that blow under minor surge conditions. However, in order to reduce truck rolls while still offering surge protection, the fuses were changed to a 4 Amp Slow Blow Fuse. 

What to do now?
At Tsp1/CT3H sites fitted with a Surge Protection Unit that does not blow fuses, no action is required.

At Tsp1/CT3H sites fitted with a Surge Protection Unit that has a blown fuse, replace both 2 Amp fuses with 4 Amp fuses (03501056).

Other Details
The material number for the 4 Amp M205 Slow Blow Anti-Surge Fuse is 03501056 (pack of 10 fuses).

Further deliveries of the Tsp1 / CT3H Surge Protection Unit (03501299) will be fitted with the 4 Amp M205 Slow Blow Anti-Surge Fuse.

Impact on HS&E
No impact on current HS&E requirements.

Contact for further information
Tom Vucetic

Telstra Payphone Services

Technical Support

02 9329 0630
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