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6. PARTS LISTS AND MATERIAL NUMBERS.

6.1 INTRODUCTION

The following list consists of 

· The minimum standard for the Tsp and CT3H Payphone

· Identification List and Material Numbers for the Tsp and CT3H Payphone

6.2 MINIMUM BUILD STANDARD FOR THE Tsp AND CT3H PAYPHONE

The following tables show the minimum Payphone standard for the various Payphones.

	Material
Number
	Material Number Description
	Product Code

	035/01151
	PAYPHONE, TELSTRA SMART NO.1 TSP1
	MPP1

	035/01218
	PAYPHONE, CARD ONLY TSP2
	MPP2

	035/01588
	PAYPHONE, CARD AND COIN CT3H
	MPP3

	035/01593
	PAYPHONE, CARD ONLY CT3H
	MPP5


NOTE: The number of units required are indicated in the columns. The individual items may be delivered in packs and it is not pack numbers that are required but single units. Other components not listed in the CT3H are generic CT3 components.
	Material Number
	Material Number Description
(Recent Changes)
	MPP1
TSP
	MPP2
TSP 
(Card)
	MPP3
CT3H
	MPP5
CT3H (Card)

	035/01172
	COIN PASSAGE DEVICE, COMPLETE TSP1 (Version 4)
	1
	
	
	

	035/01183
	EPROM, MEMORY TSP1 (V2k2)
	1
	1
	1
	1

	035/01258
	LABEL, PHONE WATCH PROGRAMME TPS (new is blue)
	1
	1
	
	

	035/01270
	COVER, COIN & CARD ENTRIES E-SHUTTER TSP1
	1
	
	
	

	035/01271
	PBA, LINE CONNECTION MODEL 2 TSP1
	1
	1
	1
	1

	035/01272
	PBA, COINBOX MODEL 2 TSP1
	1
	
	1
	

	035/01273
	SEAL, FOLLOW ON BUTTON TSP
	1
	1
	1
	1

	035/01282
	SPRING, FOLLOW ON BUTTON TSP
	1
	1
	1
	1

	035/01284
	BRACKET, LOCKING BAR SUPPORT TSP
	2
	1
	
	

	035/01285
	GASKET, GLASS FRONT DOOR/DISPLAY V2 TSP1
	1
	1
	
	

	035/01287
	GASKET, TOP FRONT DOOR TSP
	1
	1
	
	

	035/01290
	MOTOR & MOUNTING, SUB-ASSY E-SHUTTER TSP
(Pt of 035/01270)
	1
	
	1
	

	035/01291
	PBA, CONTROL UNIT E-SHUTTER TSP (Pt of 035/01270)
	1
	
	1
	

	035/01292
	CABLE, PBA E-SHUTTER – LINE BOARD (Pt of 035/01270)
	1
	
	
	

	035/01297
	LOCK, E-SHUTTER MECHANISM
	1
	
	1
	

	035/01299
	SURGE PROTECTION UNIT, TSP
	1
	1
	1
	1

	035/01575
	RAMP, COIN REFUND SS CT3H
	
	
	1
	

	035/01576
	HOPPER, COIN REFUND CUP CT3H
	
	
	1
	


	Material Number
	Material Number Description
(Recent Changes)
	MPP1
TSP
	MPP2
TSP 
(Card)
	MPP3
CT3H
	MPP5
CT3H (Card)

	035/01595
	HOUSING, CT3H E-SHUTTER
	
	
	1
	

	035/01596
	CABLE, CT3H E-SHUTTER EXTENSION
	
	
	1
	

	035/01597
	FUNNEL, COIN ENTRY CT3H
	
	
	1
	

	035/01599
	PLATE, PROTECTION FOLLOW ON BUTTON CT3H (will not fit recessed LCD model CT3H)
	
	
	1
	1

	035/01652
	KIT, RELOCATION SECURITY BOARD TSP
	1
	
	
	

	035/01655
	SEAL, DOOR CT3H/ROBUST TSP PACK OF 5
	
	
	1
	1

	035/01656
	TRAY, DRAIN EXTENSION TSP HANDSET CRADLE
	1
	1
	
	

	035/01657
	TRAY, DRAIN TSP KEY PAD
	1
	1
	
	

	035/01658
	SPACER, CT3H LCD 10MM GLASS (pack of 5)
	
	
	4
	4

	035/01662
	INSULATION, COIN REFUND CHUTE TSP
	1
	
	
	

	035/01663
	DRAIN, COIN ENTRY TSP                     
	1
	
	
	

	035/01664
	SHIELD, FLUID,MAINBOARD TSP              
	1
	1
	
	

	035/01152
	COVER, DISPLAY GLASS TSP1
	1
	1
	
	

	035/01154
	HANDSET, COMPLETE TSP1
	1
	1
	1
	1

	035/01156
	DIALPAD, ASSEMBLY COMPLETE TSP1
	1
	1
	1
	1

	035/01157
	PBA, MAIN BOARD TSP1 (the CT3H “Coin” must have latest ramp 035/01575 & coin refund hopper 035/01576 installed)
	1
	1
	1
	1

	035/01158
	READER, CARD WITH BEEPER TSP1
	1
	1
	1
	1

	035/01159
	PBA, CARD READER CONTROL TSP1
	1
	1
	1
	1

	035/01162
	STORE, INTERMEDIATE COIN TSP1
	1
	
	1
	

	035/01163
	PBA, DPH EMITTER E.U. TSP1
	1
	
	1
	

	035/01164
	PBA, DPH RECEIVER E.U. TSP1
	1
	
	1
	

	035/01165
	MECHANISM, COIN REFUND TSP1
	1
	
	
	

	035/01166
	VALIDATOR, COIN TSP1
	1
	
	1
	

	035/01168
	DISPLAY, VISUAL C/W CONNECTOR TSP1
	1
	1
	1
	1

	035/01170
	LOCK, LOWER ELECTRONIC DEVICE TSP1
	1
	
	
	

	035/01171
	LOCK, LOWER COMPARTMENT TSP1
	1
	
	
	

	035/01173
	CABLE, COIN MECHANISM TSP1
	1
	
	
	

	035/01174
	CABLE, LINE CIRCUIT TSP1
	1
	1
	
	

	035/01175
	CABLE, COIN PASSAGE TSP1
	1
	
	
	

	035/01176
	CABLE, NEW CALL KEY/HANG UP TSP1
	1
	1
	
	

	035/01177
	CABLE, KEYPAD TSP1
	1
	1
	
	

	035/01178
	CABLE, DISPLAY TSP1
	1
	1
	1
	1


	Material Number
	Material Number Description
(Recent Changes)
	MPP1
TSP
	MPP2
TSP 
(Card)
	MPP3
CT3H
	MPP5
CT3H (Card)

	035/01179
	CABLE, LOWER COMPARTMENT TSP1 (use 035/01652)
	1
	
	
	

	035/01180
	CABLE, EARTH CONNECTION TSP1
	1
	1
	1
	1

	035/01181
	CABLE, CARD READER TSP1
	1
	1
	1
	1

	035/01182
	MICROSWITCH, TSP1 C/W CABLE
	2
	1
	1
	1

	035/01184
	COIN BOX, PAYPHONE TSP1 COMPLETE
	1
	
	
	

	035/01186
	SWITCH, HOOK PAYPHONE TSP1
	1
	1
	2
	1

	035/01193
	MICROSWITCH, NEW CALL TSP1
	2
	1
	1
	1

	035/01194
	SAFE, COIN BOX TSP1 WITHOUT DOOR
	1
	
	
	

	035/01195
	DOOR, CASE FRONT TSP1 (2mm Door)
	1
	1
	
	

	035/01196
	CASE, REAR TSP1
	1
	1
	
	

	035/01197
	DOOR, SAFE TSP1
	1
	
	
	

	035/01198
	HOOKSWITCH CRADLE ASSY, PAYPHONE TSP1
	1
	1
	
	

	035/01199
	BUTTON ASSEMBLY, FOLLOW-ON PAYPHONE TSP1 (contains 03501273 & 03501282)
	1
	1
	1
	1

	035/01202
	KIT, EXTENSION PAD & SCREW SAFE BAR TSP1
	1
	
	
	

	035/01204
	PLATE, LOCKING SAFE TSP1
	1
	
	
	

	035/01207
	HINGE, DOOR COIN SAFE COMPARTMENT TSP1
	1
	
	
	

	035/01208
	CABLE ASSY, PBA TO COIN BOX SOCKET TSP1
	1
	
	
	

	035/01210
	CABLE ASSY, COINSAFE SOLENOID TO PBA TSP1
	1
	
	
	

	035/01211
	HINGE SET, UPPER DOOR COMPART TSP1
(Comes with 2mm Door) (Use 035/01660 for Robust)
	1
	1
	
	

	035/01212
	PLATE, LOCKING UPPER DOOR COMPART TSP1
(Comes with Door)
	1
	1
	
	

	035/01213
	FRAME,MOUNTING PLASTIC FOR LCD TSP1
	1
	1
	1
	1

	035/01214
	POST, MOTHER BOARD TO FRONT DOOR TSP1
	1
	1
	
	

	035/01216
	FRAME, MOUNTING CARD READER TSP1
	1
	1
	
	

	035/01219
	FRAME, MOUNTING ESCROW/VALIDATOR TSP1
	1
	
	
	

	035/01232
	GASKET, HINGE TOP DOOR TSP1
	1
	1
	
	

	035/01233
	GASKET, HINGE TOP COMPARTMENT TSP1
	1
	1
	
	


	Material Number
	Material Number Description
(Nominal)
	MPP1
TSP
	MPP2
TSP 
(Card)
	MPP3
CT3H
	MPP5
CT3H (Card)

	035/01234

035/01236

035/01237

035/01238

035/01239

035/01240

035/01241

035/01242
	LOCK, UPPER COMBINATION TSP1 (State Dependant)

NSW – Light Blue

VIC – Dark Blue

QLD - Bronze

WA - Mauve

SA - Green

TAS - Orange

NT - Grey

NAVY - Black
	1
	1
	
	

	035/01235
	DOOR, COIN REFUND MECHANISM TSP1
(Part Of 035/01165)
	1
	
	
	

	035/01243
	PBA, MEMORY EXPANSION - MOTHER BOARD TSP1
	1
	1
	1
	1

	035/01245
	BUSH, HANDSET INSERT TSP1
	1
	1
	1
	1

	035/01249
	COVER, METAL REAR INSTRUCTION PANEL TSP1
	1
	1
	
	

	035/01250
	GROMMET, UPPER COMPARTMENT BASE TSP1
	1
	
	
	

	035/01252
	RAMP, COIN REFUND TSP1
	1
	
	
	

	035/01253
	TRAY, DRAIN - CARD READER TSP1
	1
	1
	
	

	035/01254
	CONVERSION KIT, TSP1 TO TSP2 CARD ONLY
	
	1
	
	

	035/01255
	TRAY, DRAIN FOLLOW ON TSP1
	1
	1
	
	

	035/01256
	PLATE, BLANK OFF EXTERNAL JACK TSP1
	1
	1
	
	

	035/01257
	CLIP, HANDSET RETAINING TSP1
	1
	1
	1
	1

	035/01260
	FRAME, MOUNTING PLASTIC - INSTR PLATE TSP
	1
	1
	
	

	035/01261
	SPACER A, LATCH ASSEMBLY LOWER CASE TSP1
	1
	
	
	

	035/01262
	SPACER B, LATCH ASSEMBLY LOWER CASE TSP1
	1
	
	
	

	035/01263
	SPACER C, LATCH ASSEMBLY LOWER CASE TSP1
	1
	
	
	

	035/01264
	BORDER, TELSTRA FOR TSP LCD DISPLAY
	1
	1
	
	

	035/01266
	MOUNTING KIT, STANDARD SECURITY
	1
	1
	
	

	035/01267
	KIT, SECURITY LOWER COMPARTMENT TSP1
(Must be used when mounting phone in FLPC only)
	1
	
	
	

	035/01274
	KIT, LOCK ANTI-INTRUSION TSP
	2
	1
	
	

	035/01275
	PROTECTOR, LOCK UPPER & LOWER TSP
	2
	1
	
	

	035/01276
	GASKET, E-SHUTTER/DOOR NEOPRENE TSP
	1
	1
	
	

	035/01280
	FUNNEL, COIN VALIDATOR TSP 
	1
	
	1
	


	Material Number
	Material Number Description
(Nominal)
	MPP1
TSP
	MPP2
TSP 
(Card)
	MPP3
CT3H
	MPP5
CT3H (Card)

	035/01379
	MICROCHIP, SECURITY ACCESS MODUL EUROCHIP
	1
	1
	1
	1

	035/01557
	SPACER, HOPPER COIN REFUND SHUTE CT3H
	
	
	1
	

	035/01558
	SPACER, CIRCUIT BOARD CT3H
	
	
	1
	1

	035/01559
	GASKET, CARD FACIA CT3H
	
	
	1
	1

	035/01560
	GASKET, KEYPAD FACIA CT3H
	
	
	1
	1

	035/01561
	CABLE ASSY, EXTENSION H/SET-M/BOARD CT3H
	
	
	1
	1

	035/01562
	CABLE ASSY, LINE BOARD TO MAIN BOARD CT3H
	
	
	1
	1

	035/01563
	CABLE ASSY, SWITCH HOOK TO KEYPAD CT3H
	
	
	1
	1

	035/01564
	BRACKET, SUPPORT UPPER ALUMINIUM CT3H
	
	
	1
	1

	035/01565
	REST, MAIN BOARD NYLON CT3H
	
	
	1
	1

	035/01566
	CABLE ASSY, COIN BOX PCA TO MICRO-SW CT3H
	
	
	1
	

	035/01567
	CABLE ASSY, ESCROW TO MAIN BOARD CT3H
	
	
	1
	

	035/01569
	CABLE ASSY, EARTH CASE TO DOOR CT3H
	
	
	1
	1

	035/01570
	FACIA, CARD ENTRY WITH CUTOUT SS CT3H
	
	
	1
	1

	035/01571
	BRACKET, MOUNTING CARD READER CT3H
	
	
	1
	1

	035/01573
	RAMP, COIN COLLECTION SS CT3H
	
	
	1
	

	035/01574
	HOPPER, COIN C/W DPH SPACERS CT3H
	
	
	1
	

	035/01577
	CUP, COIN REFUND SS CT3HI (depending on case type)
	
	
	1
	

	035/01579
	BRACKET, MOUNTING ESCROW CT3H
	
	
	1
	

	035/01580
	CRADLE, HANDSET CT3H
	
	
	1
	1

	035/01581
	FACIA, KEYPAD MOUNT TO DOOR SS CT3H
	
	
	1
	1

	035/01582
	BRACKET, MOUNTING LOWER MAIN BOARD CT3H
	
	
	1
	1

	035/01583
	BRACKET, MOUNTING UPPER MAIN BOARD CT3H
	
	
	1
	1

	035/01585
	CLAMP, CABLE RIBBON CT3H
	
	
	3
	3

	035/01586
	LEVER, SWITCH HOOK CT3H
	
	
	1
	1

	035/01587
	BRACKET,MICROSWITCH SWITCH HOOK CT3H
	
	
	1
	1

	035/01589
	CABLE ASSY, COIN BOX PCA TO COINSAFE M/SW
	
	
	1
	

	035/01590
	CUP, COIN REFUND SS CT3HE (depending on case type)
	
	
	1
	

	035/01591
	CABLE ASSY, COIN BOX PCA TO MAIN BRD CT3H
	
	
	1
	

	035/01594
	KIT, CARD ONLY CT3H
	
	
	
	1

	035/01641
	PANEL, GLASS LCD TSP (comes with 3mm gasket, longer screws, spacers and O-rings) Note the recessed LCD CT3H payphones require 035/02005 Lexan display protector. (not used in Robust Tsp)
	1
	1
	1
	1


	Material Number
	Material Number Description
(Nominal)
	MPP1
TSP
	MPP2
TSP 
(Card)
	MPP3
CT3H
	MPP5
CT3H (Card)

	035/01643
	PANEL, GLASS LCD ROBUST TSP
(Robust phone Only)
	1
	
	
	

	035/01645
	POST,SUPPORT MEMORY EXPANSION PK10
	1
	1
	1
	1

	035/01646
	POST, SUPPORT E-SHUTTER CNTRL BD PK10
	1
	
	1
	

	035/01647
	CLAMP, RIBBON CABLE CARDREADER PK10
	1
	1
	
	

	035/01648
	SPACER, ROUND LCD TSP PK10 (comes with 035/01641)
	4
	4
	
	

	035/01649
	O-RING, MAIN BOARD POST SUPPORT PK10
	1
	1
	
	

	035/01650
	O-RING, LCD MOUNTING PK10 (comes with 035/01641)
	4
	4
	4
	4

	035/01653
	BUTTON, REFUND E-SHUTTER FACIA TSP
(Pt of 035/01270)
	1
	
	
	

	035/01654
	PLATE, MOUNTING PBA E-SHUTTER CONTRL CBLE
(Comes with CT3H Housing 035/01595)
	
	
	1
	

	035/01660
	HINGE,TSP UPPER DOOR (ROBUST)
	1
	
	
	


6.3 TELSTRA SMART PAYPHONE PARTS IDENTIFICATION LIST AND MATERIAL NUMBERS

The following table shows a picture of the different parts with their material number that are required for the Tsp and CT3H type of Payphones
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Replaced by 035/01271
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New Revision 12
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	03501152

Cover, Display Glass
	03501153

PBA, Line Connection
	03501154

Handset Complete
	03501156

Dialpad, Assembly Complete
	03501157

PBA, Main Board
	03501158

Reader, Card with Beeper
	03501159

PBA, Card Reader Controller
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Only used in 1L software sites.
	[image: image9.jpg]



	[image: image10.jpg]



	[image: image11.jpg]



	[image: image12.jpg]



	[image: image13.jpg]



	[image: image14.jpg]¢
5




Use 35/01272 in lieu

	03501160

Mechanism, Coin Entry
	03501162

Store, Intermediate coin
	03501163

PBA, DPH Emitter E.U.
	03501164

PBA, DPH Receiver E.U.
	03501165

Mechanism, Coin Refund
	03501166

Validator, Coin
	03501167

PBA, Coinbox
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Version 4

New Revision 4
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	03501168

Display, Visual C/W Connector
	03501170

Lock, Lower Electronic Device
	03501171

Lock, Lower Compartement only
	03501172

Coin Passage Device, Complete
	03501173

Cable, Coin Mechanism
	03501174

Cable, Line Circuit
	03501175

Cable, Coin Passage
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	Replaced by 03501652 

Deleted item
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	03501176

Cable, New Call

Key / Hang Up
	03501177

Cable, Keypad
	03501178

Cable, Display
	03501179

Cable, Lower Compartment
	03501180

Cable, Earth Connection
	03501181

Cable, Card Reader
	03501182

Microswitch, Cable CW - with 2 plastic rivets
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Only used in 1L software sites

	03501183

Eprom, Memory
	03501184

Coin Box
	03501185

Adaptor, RS-232-C-TL
	03501186

Switch, Hook
	03501187

Screw Kit, Miscellaneous
	03501188

Parameter Injector,  

Data Entry Unit
	03501189

Cover, Coin Entry Mechanism
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	03501192

Key, Lock Lower
	03501193

Microswitch, New Call
	03501194

Safe, Coin Box 

Without Door
	03501195

Door Case Front 

(Viewed from rear)
	03501196

Case, Rear
	03501197

Door, Safe
	03501198

Hookswitch, Cradle Assembly
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	Replaced by 03501247 

Deleted item

1L sites only
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Only used in 1L software sites. NOT USED WITH E-SHUTTER.
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	Replaced by 03501258[image: image47.jpg]




	03501199

Button Assembly, Follow-On
	03501200

Cover, Coin & Card Entry (Aluminium)
	03501201

Push Button, Coin Refund
	03501202

Kit, Extension Pad &

Screw Safe Bar
	03501203

Conversion Kit,

Payphone Card Only
	03501204

Plate, Locking Safe
	03501205

Label, How To Use Card Only


	Replaced by 03501258 

Deleted item
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	Deleted Item

For coin/card use 035/01247, or 035/01270

For card use

035/01254
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	03501206

Label, How To Use Coin and Card
	03501207

Hinge, Door

Coin Safe Compartment
	03501208

Cable Assembly,

PBA to Coin Box Socket
	03501209

Conversion Kit,

Temporary Card Only
	03501210

Cable Assembly,

Coin Safe Solenoid to PBA
	03501211

Hinge set Upper Door,

Compart MPP1
	03501212

Plate, Locking upper

Compart MPP1
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	Deleted item. 

Replaced by

03501247

03501270
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	Deleted item. 

Replaced by 03501248
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	03501213

Frame, Mounting Plastic For LCD
	03501214

Post, Mother Board

To Front Door
	03501215

Plate, Coin Entry Protection
	03501216

Frame, Mounting Card Reader
	03501217

Clamp, Coin Entry Face Plate
	03501218

Payphone, Card Only
	03501219

Frame, Mounting

Escrow/Validator
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-25TAS Orange
-26NT Grey

-27 Navy Black
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	Deleted Item
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	03501220-27

Key, Lock Upper
	03501228

Kit, Arm & Spring

Switch Hook Assy
	03501229

Wire, Safety Coinsafe To Door 
	03501230

Coin Box Lid,

Metal Payphone
	03501231

Coin Box, Bottom 
	03501232

Gasket, Hinge Door
	03501233

Gasket, Hinge Top

Compartment
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	Deleted item
	[image: image67.jpg]



	[image: image68.jpg]



Only used in 1L software sites. Replaced by 35/1270
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Only used in 1L software sites. Replaced by 35/1270

	03501234, 36-42

Lock Upper Combination
	03501235

Door, Coin Refund Mechanism
	03501243

PBA, Memory Expansion

- Mother Board
	03501244

Gasket, Glass Front 

Door / Display
	03501245

Bush, Handset Insert
	03501246

Cover, Metal Coin

Entry Mechanism
	03501247

Cover, Coin Card

Entries Stainless Steel
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Only used in 1L software sites. Replaced by 35/1270
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	03501248

Clamp, Heavy Duty

Fascia Top Door
	03501249

Cover, Rear

Instruction Panel
	03501250

Grommet, Upper

Compartment Base
	03501251

Bracket, Anchor 

Handset Cable
	03501252

Ramp, Coin Refund
	03501253

Tray, Drain 

–  Card Reader
	03501254

Conversion Kit, Amper

Payphone Card Tsp2
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	03501255

Tray, Drain Switchook
	03501256

Plate, Blank Off External Jack
	03501257

Clip, Handset Retaining
	03501258

Label, Phone Watch
	03501259

Kit Solenoid / Lock Plate
	03501260

Frame Mounting Plastic

Instruction Plate
	03501261

Latch Assembly,

Lower Case Spacer ‘A’
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	No Photo Available

2 x Knurled nuts,

 2 x M8x50mm S/S Soc Button Hd Screws,

 2 x Large series 316 S/S Washers,

 2 x M5 S/S Pin Plugs,

 2 x e-Clips
	No Photo Supplied

	03501262

Latch Assembly,

Lower Case Spacer ‘B’
	03501263

Latch Assembly,

Lower Case Spacer ‘C’
	03501264

Border, Display
	03501265

Microswitch, Cradle
	03501266

Mounting Kit, Standard Security
	03501267

Lower Compartment 

Security Kit
	03501268

TSP Safe, Complete
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Only used in 1L software sites. Replaced by 35/1270
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	03501269

Spacer, Coin Entry TSP


	03501270

Cover, Coin & Card Entries 

E-Shutter TSP1
	03501271

PBA, Line Connection  Model 2 TSP1
	03501272

PBA, Coin Box Model 2 TSP1
	03501273

Seal, Follow On Button TSP1
	03501274 

Kit, Lock Anti Intrusion


	03501275

Protector, TSP Lock Upper  & Lower
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4 per pack
	Deleted Item
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	Deleted item - use 35/01652 in lieu
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	Deleted item
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	03501276

Gasket E-Shutter/Door

Neoprene TSP
	03501277

Protector Escrow TSP1
	035/01278

Clip, Card Reader Tray TSP
	03501279

Protector, Lower Compartment Security Board
	03501280

Funnel Coin Validator TSP1
	03501281

Plug, Validator Shock 

Protector
	03501282

Spring Follow On Button TSP


	Deleted item
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10 per pack
	Not Approved 
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5 per pack
	Refer 035/01183
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	03501283

Clamp Cardreader  TSP
	03501284

Bracket, Locking Bar SupportTSP
	035/01285

Gasket, Front Door/Dsiplay V2 TSP
	035/01286

Mechanism, Coin Handling ASE TSP
	035/01287

Gasket, Top Front Door TSP
	035/01288

Eprom, Blank TSP – Pack Of 12
	035/01289

Cover, Facia E-Shutter TSP
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	Deleted Item

Replaced by 035/01272 & 035/01183.

	035/01290

Motor & Mounting, Sub-Assembly E-Shutter TSP
	035/01291

PBA, Control Unit E-Shutter TSP
	035/01292

Cable, PBA E-Shutter – Line  Board TSP
	035/01293

Kit, Mtg Upper Rear Case TSP - 2 per kit
	035/01294

Washer, Spring M5 SS TSP
	035/01295

Pinplug, M5 S/S to suit M8 hex sockethead
	035/01296

PBA, Coin Box & V2H6 Eprom Tsp
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	035/01297

Lock, E-Shutter Mechanism
	035/01298

Strip, Abrasive 3M Trizact
	035/01299

Surge Protection Unit, Tsp
	035/01641

Panel, Glass LCD Tsp (10mm)
	035/01643

Panel, Glass LCD Robust Tsp (6mm)
	035/01644

PBA, Line Build Out Resistors Tsp/Ct3H
	035/01645

Post, Support Memory Expansion Pk 10
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	035/01646

Post, Support E-Shutter Control Board Pk 10
	035/01647

Clamp, Ribbon Cable Cardreader Pk 10
	035/01648

Spacer, Round LCD Tsp 

Pk 10
	035/01649

O-Ring, Main Board Post Support Pk 10
	035/01650

O-Ring, LCD Mounting 

Pk 10
	035/01652

Kit, Relocation Security Board, Tsp
	035/01653

Button, Refund E-Shutter Facia Tsp
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	035/01656

Tray, Drain Extension Tsp Handset Cradle
	035/01657

Tray, Drain Tsp Keypad
	035/01659

Notice, Payphone Fault Codes 
	35/01660

Hinge, Tsp upper door (Robust)
	
	35/01662

Insulation, Coin Refund Chute Tsp
	35/01663

Drain, Coin Entry Tsp
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	35/01664

Shield, Fluid,Mainboard Tsp
	
	
	
	
	
	


6.4 TELSTRA CT3H PAYPHONE PARTS IDENTIFICATION LIST AND MATERIAL NUMBERS
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	035/01557

Spacer, Hopper Coin refund Shute CT3H
	035/01558

Spacer, Circuit Board CT3H
	035/01559

Gasket, Card Facia CT3H
	035/01560

Gasket, Keypad Facia CT3H
	035/01561

Cable Assy, Extension H/Set-M/Board CT3H
	035/01562

Cable Assy, Line Board to Main Board CT3H
	035/1563

Cable Assy, Switch Hook to Keypad CT3H
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	035/01564

Bracket, Support Upper Aluminium CT3H
	035/01565

Rest, Main Board Nylon CT3H
	035/01566

Cable Assy, Coin Box PCA to Micro SW CT3H
	035/01567

Cable Assy, Escrow to Main Board CT3H
	035/01569

Cable Assy, Earth Case to Door CT3H
	035/01570

Facia, Card Entry with Cutout SS CT3H
	035/01571

Bracket, Mounting Card Reader CT3H
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Deleted item - Replaced by35/1290, 1291, 1595, 1596 & 1597
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	035/01572

Coin Head Entry, Smart CT3H
	035/01573

Ramp, Coin Collection SS CT3H
	035/01574

Hopper, Coin C/W DPH Spacers CT3H
	035/01575

Ramp, Coin Refund  CT3H
	035/01576

Hopper, Coin Refund Cup CT3H
	035/01577

Cup, Coin Refund SS CT3Hi
	035/01579

Bracket, Mounting Escrow CT3H
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	035/01580

Cradle, Handset CT3H
	035/01581

Facia, Keypad Mount to Door SS CT3H
	035/01582

Bracket, Mounting Lower Main Board CT3H
	035/01583

Bracket, Mounting Upper Main Board CT3H
	035/01585

Clamp, Cable Ribbon CT3H
	035/01586

Lever, Switch Hook CT3H
	035/01587

Bracket, Microswitch Hook CT3H
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	No Photo 

Supplied
	No Photo 

Supplied
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	035/01588

Payphone Card & Coin CT3H
	035/01589

Cable Assy, Coin box PCA  to Coin Safe M/SW CT3H
	035/01590 

Cup, Coin Rrefund SS CT3HE
	035/01591

Coin Box PCA to main board CT3H
	035/01592

Payphone (Complete),

Coin Only CT3H
	035/01593

Payphone (Complete),

Card Only CT3H
	035/01594

Kit, Card Only CT3H
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	035/01595

Housing, CT3H E‑Shutter
	035/01596

Cable, CT3H E‑ShutterExtension
	035/01597

Funnel, Coin Entry CT3H (pack of 5)
	035/01598

PBA, Main Board CT3H

Use if refund ramp assy is not modified 
	035/01599

Plate, Protection Follow On Button CT3H
	035/01654

Plate, Mounting PBA E-Shutter Control Cable
	035/01655

Seal, Door CT3H/Robust Tsp pack of 5
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	035/01658

Spacer, CT3H LCD 10mm Glass
	
	
	
	
	
	


6.5 GLOSSARY OF TERMS

	TERM
	Definition

	BPS
	Bits Per Second.  A measure of communication speed on serial links.

	Chargeable Number
	A number dialled by the user that will result in a deduction of available credit on CSA.

	CIE
	Card Information Entry. This is the DEU switch setting used for setting Card Reader Initial Parameters.

	Collection
	The action of reduction of credit from the Phonecard or causing coins to fall into the coin safe.

	CPU
	Central Processing Unit. The part of a computer or electronic device that executes programs. CPU often refers to the microprocessor chip.

	CREDIT
	In general, the amount of credit available for making chargeable calls. Credit can be any of the following types:

Card Credit. This is the total amount of credit read from the Phonecard and stored in memory.

Suspended Credit (also known as Suspense Credit). The value of coins which have been inserted but not yet collected. These coins may be collected as the call proceeds, or they may be returned when the caller hangs up.

Logic Credit. This is the amount transferred from the Suspended Credit as coins are collected. For example, if a 20¢ coin is collected during a call, the amount of Suspended Credit is reduced by 20¢, and the amount of Logic Credit is increased by 20¢.

Total Credit. This is the total of the Suspended Credit and the Logic Credit.

	CSA
	Called Subscriber Answer. Line Reversal and meter pulse received from the exchange upon B party answer. (Meter pulse must be received within 3.3 seconds of line reversal).

	CTA
	Coin Tin Full Alarm. This is an alarm transmitted to the MTMS when a pre-defined amount of cash has been collected by the Tsp1. Once the CTA has been registered, no further coin-operated calls can be made until the alarm is cleared. (ie. until the coin box is emptied) (See CTW.)

	CTC
	Coin Tin Contents.

	CTS
	Clear To Send. A signal used for handshaking in serial communication.

	CTW
	Coin Tin Warning. This is an alarm transmitted to the MTMS when a pre-defined amount of cash has been collected by the Tsp1. Unlike the CTA, this is a warning message only, and operation can continue as normal. See CTA.

	Decadic
	A system which uses pulses to identify key presses.  Now being replaced by DTMF.

	Default Timer
	If meter pulses are not received during a timed call, the Tsp1 will revert to default metering. The Default Time is the time between these automatic metering pulses. The default time can be downloaded from the MTMS.

	Dial Analysis
	The ability of the Payphone to analyse dialled digits to distinguish between non chargeable, local, STD and IDD calls.

	DIL
	Dual In Line. This describes connectors, semiconductors and other components which have two parallel rows of pins or sockets.

	DTMF
	Dual Tone Multi-Frequency. A dialling system which uses different frequencies, rather than pulses, to identify key-presses. Wherever possible, the Tsp1 should be set for DTMF rather than Decadic operation. The Maintenance Menu mode can be used to test the tones used to generate DTMF.  DTMF is also known as Voice Frequency, Tone Dialling, or Tone Sending.


	TERM
	Definition

	Earth (Metering)
	An electrical earth used in 50Hz metering.

	Earth (Protective) 
	A protective earth used to ensure that the case of the instrument is at the same potential as local earth and cannot reach dangerous potential.

	EEPROM
	Electrically Erasable Programmable Read Only Memory.  A memory chip which does not lose its memory when power is removed.  It is intended mainly for Read operations, but its contents can be electrically erased and re-programmed.

	EPROM
	Erasable Programmable Read Only Memory. A memory chip which does not lose its memory when power is removed. It is electrically programmed and is intended for Read operations. Its contents cannot be easily erased.

	Free Call
	A call for which no charge is made.

	IDD
	International Direct Dialling. The facility whereby users can obtain access to numbers in another country, without operator assistance. Formerly known as ISD (International Subscriber Dialling).

	LCD
	Liquid Crystal Display. An LCD display is used on the Tsp1 to provide customer information.

	LED
	Light Emitting Diode.

	Limited Service
	Only those emergency numbers are allowed to dialled

	Local Call
	A local call is one to a subscriber within the local service area of the calling instrument. These calls are untimed.

	MCF
	Minimum Call Fee. The minimum amount of credit which must be available before any chargeable call can be made.

	Metering Period
	The period of time (T) between metering signals subsequent to the second metering signal. Note that the first metering period from CSA  can vary between T and 2T.


	Metering Pulse
	Also known as Metering Signal. This is a signal sent from the exchange, and used for costing calls. In the case of local calls, one metering pulse is sent on CSA. In the case of STD and IDD calls, metering pulses are sent at various intervals, depending on the charge associated with the call being made. As pulses are received, the amount of available credit is reduced.  The Tsp1 can detect 50Hz, 12kHz, 16kHz (currently not used in Australia) and DC metering pulses (DC metering is rarely used).

	MTMS
	Modular Terminal Management System. A system which communicates directly with individual Tsp1 (and other) phones and which is used for statistical, management and maintenance purposes.


	Multimetering Calls
	An STD, IDD, VAS, Mobile or Community Access Call with meter pulses sent from the exchange at regular intervals during the call.

	Out of Service
	An operating mode in which a call can not be made because of a detected fault condition.

	PBA
	Printed Board Assembly. This is a Printed Circuit Board (PCB) together with all its components.

	PCB
	Printed Circuit Board.

	Phonecard
	The Telstra pre-paid Smartcard, designed to be used with the Tsp and CT3H.

	PIU
	Parameter Injection Unit. This is a device used for setting up the initial parameters for the Tsp1 and its Card Reader and for resetting parameters whenever necessary. The PIU is also used for setting parameters.


	TERM
	Definition

	PPS
	Pulses Per Second during decadic dialling.

	PTO
	Public Telephone Operator.

	RAM
	Random Access Memory. A memory chip which loses its contents when power is removed. It is used for temporary storage of data.

	RFI
	Radio Frequency Interference.

	RTS
	Request To Send. A signal used for handshaking in serial communication.

	SAM
	Security Access Module.

	Smartcard
	A programmable disposable or reusable, prepaid chip card  designed to be used with the Tsp1.

	STD
	Subscriber Trunk Dialling. The facility whereby users can obtain access by dialling to numbers in another charge area not within the local call area, without operator assistance.

	Threshold Time
	If meter pulses are not received during a timed call, the Tsp1 will revert to self-metering. The Threshold Time is the time between CSA and the beginning of self-metering pulse.

	TRC
	Telecommunications Reference Conductor.

	Tsp
	A Telstra smart payphone which is capable of accepting all Australian coin types and Telstra pre-paid Phonecards (Smartcard).

	VF
	Voice Frequency. This is an old term for DTMF.

	WDT
	WatchDog Timer. If the main CPU enters a "runway" or other abnormal operating state, the WDT causes a reset signal to be output automatically and returns the CPU to its normal operation.
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