m-Qube Connectivity Provisioning Worksheet


m-Qube Connectivity Provisioning Worksheet
 v 1.4
Please complete all shaded boxes and email to connectivitygroup@m-qube.com
Contact Information

Company Name: 
   
Address: 



Project Manager

Name:
Desk Phone:

Email:
Mobile Phone:

Technical/Operations Contact (24x7)

Name:
Desk Phone:

Email:
Mobile Phone:

VPN/Networking Technical Contact (24x7)

Name:
Desk Phone:

Email:
Mobile Phone:


Program Information

Will your program use Premium SMS Messaging: 
   
Will your program use Wap Push: 




Complete this page if you are requesting a
Web Services Connection
	
	m-Qube Production
	m-Qube Test
	Customer Production
	Customer Test

	m-Qube will send MO messages to customer URL*
	N/A
	N/A
	Insert your URL here
	Insert your URL here

	Use either URL to send MT Msgs To subscriber **
	http://studio.mqube.us/campaignapp/services/MessagingWS?WSDL (Via SOAP)

http://studio.mqube.us/campaignapp/post/sendMessage? (via HTTP)
	http://studio.m-qube.us/campaignapp/services/MessagingWS?WSDL (Via SOAP)

http://studio.m-qube.us/campaignapp/post/sendMessage? (via HTTP)
	N/A
	N/A


*  Same URLs are available via SSL if desired

**  Please also specify additional parameters required from m-Qube (Refer to m-Qube API spec)
Please enter all test phone numbers below 
Only the phone numbers listed below will be available to test your application until it has passed our Certification Department.  Once it has passed and we have internally launched your application, end users will be able to access it.
	PHONE NUMBER 
	CARRIER

	
	

	
	

	
	

	
	

	
	

	
	

	
	

	
	


Complete this page if you are requesting an
SMPP Connection

(An optional VPN feature is available in Production only)

	
	m-Qube Production
	m-Qube Test
	Customer Production
	Customer Test

	EXTERNAL IP address of your firewall 
	
	
	
	

	VPN IP address
	64.14.95.6
	64.14.95.6
	
	

	Firewall Version and Model
	Cisco Pix 6.3
	Cisco Pix 6.3
	
	

	Encryption type
	3DES-md5
	3DES-md5
	3DES-md5
	3DES-md5

	Preshared key
	mQ&b3s3c
	mQ&b3s3c 
	mQ&b3s3c
	mQ&b3s3c

	Diffie helman Group
	2
	2
	2
	2

	Renegotiate phase 1
	28800
	28800
	28800
	28800

	SMPP Version
	3.4
	3.4
	
	

	SMPP host (Complete this row only if a VPN connection is NOT desired)
	anakin.mqube.us
	ilum.m-qube.us
	
	

	Do you want separate transmit/receive binds or a single transceiver bind?
	
	
	
	

	Application port
	16911
	16912
	N/A
	N/A

	Customer SMPP Server Vendor or Client Library Vendor
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